mat-files:
burst2.mat 		ADV-Vector data processed into wave height. Unit: m.
landerDAY.mat		Lander deployment start- and enddata of de lander deployments in matlab-time. 
sallspmchla.mat		Processed SPM and CHL-a data at 4 levels: 0.3 mab, 0.8 mab, 1.4 mab, 2.0 mab. Processing steps: checked, interpolated and smoothed. Units: mg/l and microgram/l. 
trfli.mat 		Transport per time-frame and per sigma-layer (20 layers), interpolated and smoothed. 
TR12.mat		Tide-averaged values. Tides are determined by 0-crossings of current. 

m-scripts:
transport_calculation_frame.m
	file that generates trfli3.mat from ADCP (ADCPVf.mat), ADV (burst2.mat) and SPM (sallspmchla.mat)
VariablesTR12.m
	file that calculates various transport variables per tidal cycle.
	